p4dpdk multiseg rx/tx loop
nat and pbr config to have reindex
bridge security from dhcp, slaac, whatever server
bgp optimal route reflection
bgp peer autoconfig
bgp layer2 flowspec
bgp strict bfd mode
bgp signed path
traffic through bgp sr-policy
traffic through bgp nsh
parse privilege levels from tacacs
ldap client, server
trustpoint for certificates
dhcp relay support
tcp selective ack
xot, x75 switching
ilnp (rfc6740)
lisp4, lisp6
rift4, rift6
l2vpn for isis
hip (rfc4423)
more show commands
more clear commands
more interactive tools
more features with clean implementation
more randomizers
x25
default vrf for show commands
