check lsrp4
 command sho ipv4 lsrp 1 spf | include able
 description ipv4 lsrp reachability
 error-text nodes changed
 train
 exit

check lsrp6
 command sho ipv6 lsrp 1 spf | include able
 description ipv6 lsrp reachability
 inherit lsrp4
 exit
