hostname sid
buggy
password-encrypt $v10$czNjcjN0
enable $V10$LmUbNUUefDFvI3E6XXkWBU4uX3V1JHM3ZGRHEnJQESRJTQZ0MxQ3dDk2Iks3J2xbmoBU5FUKnZ2TeM5wjTkv6kckltWXdlCgjoLmByDO
banner encoded  
!
logging tracestop
logging milliseconds
logging buffered debug 10240
logging file debug zzz.log
logging syslog debug system 100.100.3.10 100.100.3.4
logging irc debug irc.mchome.nop.hu #routers
!
crypto rsakey rsa import $w10$ 
!
crypto dsakey dsa import $w10$ 
!
crypto ecdsakey ecdsa import $w10$N3OLUiq1x+Jok7NWfAzVIVI3eVUquH4ToWzkAx73xvqx/eRdznuSwWXSoCrbKEA4aw4/mogfgEXbiEXunbIrVUx857RvCyetdoKgPCZDWpTws74TTNdA6NCZGUnC1L7QhbrhBKvMuTNf4/6VPlUWiw==
!
crypto mldsakey mldsa import $w10$ 
!
crypto certificate dsa import dsa dsa $w10$ 
!
crypto certificate ecdsa import ecdsa ecdsa $w10$N3+SZCatxfNCk71haWzGFUIaSCJtj30H0VflBHqp29SJ4I1exDiewmXUmBLcOD0maTg1q70Lg3L6nSylu+E4W2lwloh4LSP+VY3Mfj5/ad/q+8FSN+VVm/OqNz/e0dqay/6ofOa29AMStZHiei9TxTvsFfSS3G39EK01bz/4zJ7jBTQo0uYZGn1kMfqU3qNvnsEAa32e9x5OEV3ifkzeD3tb8CfCkjF4k2d39JSe0ffMkEH4nQ2DdKzLNvhQA0loCvcHcniK+RMwn7HkG/6zhiuA/nYJEs0J7JujQVlIYbPX8+QmgYcM0guG8HElEZY5hHwS7dnroQWeQdAkA6J5Fyy+9u38eacr8/13FkuzexRgdirju2jfOC5A7jq74hHrTwkigfKGxEGOMm60BlJQfgq/TVUGl9gv6eyVPnD+GmLFY+D9KnoQWxTC16oSAcUQ
!
crypto certificate mldsa import mldsa mldsa $w10$ 
!
crypto certificate rsa import rsa rsa $w10$ 
!
aaa userlist access
 log-failure
 log-error
 log-success
 log-password
 username *
 username * anypass
 username * anykey
 username * privilege 1
 username mc36
 username mc36 password $w10$HFepawSJgqct0vAiKD2PVg==
 username mc36 pubkey  
 forbidden ^show.*config$
 forbidden ^show config.*$
 allowed show .*
 allowed view .*
 allowed watch .*
 allowed display .*
 allowed differs .*
 allowed terminal .*
 allowed test .*
 allowed game .*
 allowed send .*
 allowed terminal .*
 allowed flash .*
 allowed tmux .*
 allowed enable
 allowed disable
 allowed exit
 allowed logout
 allowed configure terminal
 allowed interface .*
 allowed description .*
 allowed telnet .*
 exit
!
aaa radius rad
 secret $w10$GV+pcgTkgqct0vAiKD2PVg==
 server 100.100.3.227
 exit
!
aaa tacacs tac
 secret $w10$GV+pcgTkgqct0vAiKD2PVg==
 server 100.100.3.227
 exit
!
script logger
 sequence 10 exec "test logging info someone from $remote hit the script"
 sequence 20 puts "just some text"
 stop
 exit
!
prefix-list def4
 sequence 10 permit 0.0.0.0/0 ge 0 le 0
 exit
!
prefix-list def6
 sequence 10 permit ::/0 ge 0 le 0
 exit
!
prefix-list nht4
 sequence 10 permit 100.100.0.0/16 ge 32 le 32
 exit
!
prefix-list nht6
 sequence 10 permit 2001:db8::/32 ge 128 le 128
 exit
!
route-policy nht
 sequence 10 if distance 70
 sequence 20   pass
 sequence 30 else
 sequence 40   drop
 sequence 50 enif
 exit
!
bundle 1
 loadbalance all
 exit
!
bridge 1
 rd 65535:1
 rt-import 65535:1
 rt-export 65535:1
 mac-learn
 private-bridge
 exit
!
bridge 2
 rd 65535:2
 rt-import 65535:2
 rt-export 65535:2
 mac-learn
 private-bridge
 exit
!
bridge 3
 rd 65535:1
 rt-import 65535:1
 rt-export 65535:1
 mac-learn
 private-bridge
 exit
!
bridge 4
 rd 65535:2
 rt-import 65535:2
 rt-export 65535:2
 mac-learn
 private-bridge
 exit
!
bridge 9
 rd 65535:103
 rt-import 65535:103
 rt-export 65535:103
 mac-learn
 mac-move
 exit
!
vrf definition bvi
 rd 65535:2
 exit
!
vrf definition dn42
 rd 65535:42
 rt4import 65535:42
 rt4export 65535:42
 rt6import 65535:42
 rt6export 65535:42
 mdt4 mldp
 mdt6 mldp
 exit
!
vrf definition freenet
 exit
!
vrf definition rtbh
 rd 65535:666
 rt4import 65535:666
 rt4export 65535:666
 rt6import 65535:666
 rt6export 65535:666
 exit
!
vrf definition v1
 rd 1:1
 rt4import 1:1
 rt4export 1:1
 rt6import 1:1
 rt6export 1:1
 exit
!
vrf definition v2
 rd 1:2
 rt4import 1:2
 rt4export 1:2
 rt6import 1:2
 rt6export 1:2
 label4mode per-prefix
 label6mode per-prefix
 exit
!
vrf definition v3
 rd 1:3
 rt4import 1:3
 rt4export 1:3
 rt6import 1:3
 rt6export 1:3
 label4mode per-prefix
 label6mode per-prefix
 exit
!
vrf definition v4
 rd 1:4
 rt4import 1:4
 rt4export 1:4
 rt6import 1:4
 rt6export 1:4
 label4mode per-prefix
 label6mode per-prefix
 exit
!
vrf definition v5
 rd 1:5
 rt4import 1:5
 rt4export 1:5
 rt6import 1:5
 rt6export 1:5
 label4mode per-prefix
 label6mode per-prefix
 exit
!
vrf definition v6
 rd 1:6
 rt4import 1:6
 rt4export 1:6
 rt6import 1:6
 rt6export 1:6
 label4mode per-prefix
 label6mode per-prefix
 exit
!
vrf definition v7
 rd 1:7
 rt4import 1:7
 rt4export 1:7
 rt6import 1:7
 rt6export 1:7
 label4mode per-prefix
 label6mode per-prefix
 exit
!
vrf definition v8
 rd 1:8
 rt4import 1:8
 rt4export 1:8
 rt6import 1:8
 rt6export 1:8
 label4mode per-prefix
 label6mode per-prefix
 exit
!
vrf definition v9
 rd 1:9
 rt4import 1:9
 rt4export 1:9
 rt6import 1:9
 rt6export 1:9
 label4mode per-prefix
 label6mode per-prefix
 exit
!
vrf definition vpn
 rd 65535:1
 rt4import 65535:1
 rt4export 65535:1
 rt6import 65535:1
 rt6export 65535:1
 mdt4 mldp
 mdt6 mldp
 exit
!
router blackhole4 1 vrf rtbh
 exit
!
router blackhole6 1 vrf rtbh
 exit
!
router lsrp4 1 vrf v1
 router-id 100.100.3.227
 refresh 600000
 lifetime 2147483000
 ha-mode
 spf-log 500
 spf-bidir
 spf-ecmp
 suppress-prefix
 segrout 300 227
 bier 256 300 227 0
 justadvert loopback0
 ecmp
 exit
!
router lsrp6 1 vrf v1
 router-id 100.100.3.227
 refresh 600000
 lifetime 2147483000
 ha-mode
 spf-log 500
 spf-bidir
 spf-ecmp
 suppress-prefix
 segrout 300 227
 bier 256 300 227 0
 justadvert loopback0
 ecmp
 exit
!
router logger4 1 vrf v1
 flapstat
 redistribute lsrp4 1
 exit
!
router logger4 65535 vrf v1
 flapstat
 redistribute bgp4 65535
 exit
!
router logger6 1 vrf v1
 flapstat
 redistribute lsrp6 1
 exit
!
router logger6 65535 vrf v1
 flapstat
 redistribute bgp6 65535
 exit
!
interface template1
 description core links
 monitor-buffer 10240000
 lldp enable
 cdp enable
 cdp odr4 100.100.1.246
 cdp odr6 2001:db8:1123::91
 ptp enable
 ptp receive
 carrier-delay 123
 sgt enable
 vrf forwarding v1
 ipv4 address dynamic 255.255.255.252
 ipv4 host-watch appear logger change logger disappear logger
 ipv4 srh enable
 ipv4 nsh enable
 ipv4 ptp enable
 ipv4 ptp receive
 ipv4 bfd 1000 3000 3
 ipv4 pim enable
 ipv4 pim bier-tunnel 227
 ipv4 pim join-source loopback0
 ipv6 address dynamic ffff:ffff:ffff:ffff::
 ipv6 host-watch appear logger change logger disappear logger
 ipv6 srh enable
 ipv6 nsh enable
 ipv6 ptp enable
 ipv6 ptp receive
 ipv6 bfd 1000 3000 3
 ipv6 pim enable
 ipv6 pim bier-tunnel 227
 ipv6 pim join-source loopback0
 polka enable 227 70000 256
 mpls enable
 mpls ldp4
 mpls ldp6
 mpls rsvp4
 mpls rsvp6
 router lsrp4 1 enable
 router lsrp4 1 dump lsrp4.log
 router lsrp4 1 accept-metric
 router lsrp4 1 bfd
 router lsrp4 1 ipinfo pmtud 768 1024 666
 router lsrp4 1 dynamic-metric mode inband
 router lsrp4 1 dynamic-metric size 4
 router lsrp4 1 dynamic-metric ignore 2
 router lsrp6 1 enable
 router lsrp6 1 dump lsrp6.log
 router lsrp6 1 accept-metric
 router lsrp6 1 bfd
 router lsrp6 1 ipinfo pmtud 768 1024 666
 router lsrp6 1 dynamic-metric mode inband
 router lsrp6 1 dynamic-metric size 4
 router lsrp6 1 dynamic-metric ignore 2
 shutdown
 no log-link-change
 exit
!
interface loopback0
 description management
 vrf forwarding v1
 ipv4 address 100.100.3.227 255.255.255.255
 ipv6 address 2001:db8:1101::227:227 ffff:ffff:ffff:ffff:ffff:ffff:ffff:ffff
 template template1
 no shutdown
 exit
!
interface loopback42
 description dn42.net
 vrf forwarding dn42
 ipv4 address 172.23.215.130 255.255.255.255
 ipv6 address fd40:cc1e:c0de::fffd ffff:ffff:ffff:ffff:ffff:ffff:ffff:ffff
 no shutdown
 no log-link-change
 exit
!
interface loopback65535
 description vpn
 vrf forwarding vpn
 ipv4 address 172.16.27.4 255.255.255.255
 ipv6 address fd42:1234::4 ffff:ffff:ffff:ffff:ffff:ffff:ffff:ffff
 no shutdown
 no log-link-change
 exit
!
interface bundle1
 description uplink
 no shutdown
 no log-link-change
 exit
!
interface bundle1.227
 description uplink
 vrf forwarding v1
 ipv4 address 100.100.1.246 255.255.255.252
 ipv6 address 2001:db8:1123::91 ffff:ffff:ffff:ffff::
 template template1
 no shutdown
 exit
!
interface bvi1
 description vpn
 lldp enable
 cdp enable
 no shutdown
 no log-link-change
 exit
!
interface bvi2
 description vpn
 lldp enable
 cdp enable
 no shutdown
 no log-link-change
 exit
!
interface bvi3
 description vpn
 lldp enable
 cdp enable
 vrf forwarding bvi
 ipv4 address 172.16.26.4 255.255.255.0
 ipv6 address fd42:1235::4 ffff:ffff:ffff:ffff::
 no shutdown
 no log-link-change
 exit
!
interface bvi4
 description vpn
 lldp enable
 cdp enable
 no shutdown
 no log-link-change
 exit
!
interface bvi9
 description freenet
 vrf forwarding freenet
 ipv4 address dynamic dynamic
 ipv4 gateway-prefix def4
 ipv4 host-watch
 ipv4 dhcp-client enable
 ipv4 dhcp-client early
 ipv6 address dynamic dynamic
 ipv6 gateway-prefix def6
 ipv6 host-watch
 ipv6 slaac-client enable
 ipv6 prefix-suppress
 no shutdown
 no log-link-change
 exit
!
interface ethernet1
 description uplink1
 bundle-group 1
 no shutdown
 no log-link-change
 exit
!
interface ethernet2
 description uplink2
 bundle-group 1
 no shutdown
 no log-link-change
 exit
!
interface ethernet8
 description hairpin
 lldp enable
 cdp enable
 no shutdown
 no log-link-change
 exit
!
interface ethernet9
 description hairpin
 lldp enable
 cdp enable
 no shutdown
 no log-link-change
 exit
!
interface null0
 description null
 vrf forwarding v1
 ipv4 address 192.0.2.0 255.255.255.0
 ipv6 address 100:: ffff:ffff:ffff:ffff::
 no shutdown
 no log-link-change
 exit
!
router bgp4 65535 vrf v1
 local-as 65535
 router-id 100.100.3.227
 address-family unicast multicast vpnuni vpnmlt vpls evpn mdt flowspec vpnflw ovpnuni ovpnmlt ovpnflw mvpn omvpn mspw srte linkstate ouni omlt oflw osrt nsh rtfilter rpd mtree omtree spf sdwan mup omup tunnel encap
 flapstat
 nexthop route-policy nht
 nexthop prefix-list nht4
 monitor bmp p1 100.100.3.227 17971
 dump mrt bgp4.log
 !
 template r remote-as 65535
 template r local-as 65535
 template r ipinfo pmtud 512 1024 666
 template r ipinfo router4 bgp4 65535
 template r ipinfo resolve
 template r address-family unicast multicast vpnuni vpnmlt vpls evpn mdt flowspec vpnflw ovpnuni ovpnmlt ovpnflw mvpn omvpn mspw srte linkstate ouni omlt oflw osrt nsh rtfilter rpd mtree omtree spf sdwan mup omup tunnel encap
 template r distance 200
 template r connection-mode active
 template r dynamic-capability
 template r compression both
 template r additional-path-rx unicast multicast vpnuni vpnmlt
 template r additional-path-tx unicast multicast vpnuni vpnmlt
 template r update-source loopback0
 template r monitor bmp
 template r dump mrt
 template r hostname domain
 template r software
 template r extended-open
 template r extended-update
 template r ha-mode
 template r aigp
 template r entropy
 template r traffeng
 template r pmsitun
 template r connector
 template r pe-distinguisher
 template r aspath-limit
 template r nsh-chain
 template r domain-path
 template r safi-specific
 template r destination-preference
 template r bfd-discriminator
 template r tunenc
 template r attribset
 template r unknowns-out all
 template r unknowns-in all
 template r unknowns-log
 template r segrout
 template r bier
 template r leak-role attrib
 template r next-hop-capability
 template r send-community all
 !
 neighbor 100.100.3.254 template r
 !
 neighbor 100.100.3.255 template r
 !
 afi-vrf dn42 enable
 afi-vrf dn42 mvpn loopback0
 afi-vrf dn42 redistribute connected
 afi-vrf dn42 redistribute static
 afi-vrf dn42 ecmp
 !
 afi-vrf rtbh enable
 afi-vrf rtbh redistribute blackhole4 1
 !
 afi-vrf vpn enable
 afi-vrf vpn mvpn loopback0
 afi-vrf vpn redistribute connected
 afi-vrf vpn redistribute static
 !
 afi-vpls 65535:1 bridge-group 1
 afi-vpls 65535:1 update-source loopback0
 !
 afi-vpls 65535:103 bridge-group 9
 afi-vpls 65535:103 update-source loopback0
 !
 afi-evpn 2 bridge-group 2
 afi-evpn 2 bmac 006e.085c.1743
 afi-evpn 2 encapsulation pbb
 afi-evpn 2 update-source loopback0
 !
 !
 redistribute connected
 redistribute static
 ecmp
 exit
!
router bgp6 65535 vrf v1
 local-as 65535
 router-id 100.100.3.227
 address-family unicast multicast vpnuni vpnmlt vpls evpn mdt flowspec vpnflw ovpnuni ovpnmlt ovpnflw mvpn omvpn mspw srte linkstate ouni omlt oflw osrt nsh rtfilter rpd mtree omtree spf sdwan mup omup tunnel encap
 flapstat
 nexthop route-policy nht
 nexthop prefix-list nht6
 monitor bmp p1 2001:db8:1101::227:227 17971
 dump mrt bgp6.log
 !
 template r remote-as 65535
 template r local-as 65535
 template r ipinfo pmtud 512 1024 666
 template r ipinfo router4 bgp4 65535
 template r ipinfo resolve
 template r address-family unicast multicast vpnuni vpnmlt vpls evpn mdt flowspec vpnflw ovpnuni ovpnmlt ovpnflw mvpn omvpn mspw srte linkstate ouni omlt oflw osrt nsh rtfilter rpd mtree omtree spf sdwan mup omup tunnel encap
 template r distance 200
 template r connection-mode active
 template r dynamic-capability
 template r compression both
 template r additional-path-rx unicast multicast vpnuni vpnmlt
 template r additional-path-tx unicast multicast vpnuni vpnmlt
 template r update-source loopback0
 template r monitor bmp
 template r dump mrt
 template r hostname domain
 template r software
 template r extended-open
 template r extended-update
 template r ha-mode
 template r aigp
 template r entropy
 template r traffeng
 template r pmsitun
 template r connector
 template r pe-distinguisher
 template r aspath-limit
 template r nsh-chain
 template r domain-path
 template r safi-specific
 template r destination-preference
 template r bfd-discriminator
 template r tunenc
 template r attribset
 template r unknowns-out all
 template r unknowns-in all
 template r unknowns-log
 template r segrout
 template r bier
 template r leak-role attrib
 template r next-hop-capability
 template r send-community all
 !
 neighbor 2001:db8:1101::254 template r
 !
 neighbor 2001:db8:1101::255 template r
 !
 afi-vrf dn42 enable
 afi-vrf dn42 mvpn loopback0
 afi-vrf dn42 redistribute connected
 afi-vrf dn42 redistribute static
 afi-vrf dn42 ecmp
 !
 afi-vrf rtbh enable
 afi-vrf rtbh redistribute blackhole6 1
 !
 afi-vrf vpn enable
 afi-vrf vpn mvpn loopback0
 afi-vrf vpn redistribute connected
 afi-vrf vpn redistribute static
 !
 afi-vpls 65535:1 bridge-group 3
 afi-vpls 65535:1 update-source loopback0
 !
 afi-evpn 2 bridge-group 4
 afi-evpn 2 bmac 0002.4276.7a16
 afi-evpn 2 encapsulation pbb
 afi-evpn 2 update-source loopback0
 !
 !
 redistribute connected
 redistribute static
 ecmp
 exit
!
console0
 exec bells
 exec colorize header
 no exec authorization
 no login authentication
 exit
!
proxy-profile dn42
 vrf dn42
 exit
!
proxy-profile p1
 vrf v1
 source loopback0
 exit
!
proxy-profile p2
 vrf v2
 exit
!
proxy-profile p3
 vrf v3
 exit
!
proxy-profile p4
 vrf v4
 exit
!
proxy-profile p5
 vrf v5
 exit
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
translation-rule 1
 remove %20
 remove -
 remove \(
 remove \)
 replace \+36 06
 match ^sip:(?<n>[0-9]+)@(?<d>.*)$
 match ^.*<sip:(?<n>[0-9]+)@(?<d>.*)>.*$
 match ^(?<n>[0-9]+)$
 text "
 variable n
 text "
 character 32
 text <sip:
 variable n
 text @100.100.3.10>
 log
 exit
!
translation-rule 2
 match .*
 text "96" <sip:97@100.100.3.10>
 exit
!
translation-rule 3
 match ^http://(?<d>.*)\.dn42.sid.mchome.nop.hu/(?<p>.*)$
 text http://
 variable d
 text .dn42/
 variable p
 log
 exit
!
translation-rule 4
 match ^http://(?<d>.*)\.inet.sid.mchome.nop.hu/(?<p>.*)$
 text http://
 variable d
 text /
 variable p
 log
 exit
!
dial-peer 1
 match-calling .*
 match-called .*
 translate-out-calling 2
 translate-out-called 1
 port-remote 6050
 keepalive 15000
 log
 history 10
 vrf v1
 source loopback0
 myname 97
 target 2001:db8:1101::10
 max-calls-in 99
 max-calls-out 99
 protocol sip-connect
 direction both
 exit
!
!
server telnet tel vrf v1 interface loopback0
 security authentication access
 security rsakey rsa
 security dsakey dsa
 security ecdsakey ecdsa
 security mldsakey mldsa
 access-log
 access-total 128
 access-subnet 16
 access-blackhole4 1
 access-blackhole6 1
 exec timestamp
 exec bells
 exec colorize header
 exec tablemode table
 exec authorization access
 login authentication access
 login stars
 login logging
 login last global
 location
 second-port 22
 exit
!
server udptn ut vrf v1 interface loopback0
 no exec authorization
 no login authentication
 login logging
 exit
!
server rfb vnc vrf v1 interface loopback0
 no exec authorization
 no login authentication
 login logging
 exit
!
server echo e
 vrf v1
 exit
!
server discard d
 vrf v1
 exit
!
server chargen c
 vrf v1
 exit
!
server forwarder tel vrf v1 interface loopback0
 port 2323
 location
 target vrf v1
 target interface loopback0
 target address 100.100.3.227
 target port 23
 exit
!
server http web vrf v1 interface loopback0
 security rsakey rsa
 security dsakey dsa
 security ecdsakey ecdsa
 security mldsakey mldsa
 security rsacert rsa
 security dsacert dsa
 security ecdsacert ecdsa
 security mldsacert mldsa
 access-log
 access-total 128
 access-peer 16
 access-startup 10000
 second-port 443
 host * path /nfs/own/web/
 host * redir http://sid.mchome.nop.hu/
 host *.dn42.sid.mchome.nop.hu path /nfs/own/web/
 host *.dn42.sid.mchome.nop.hu reconn dn42 http://www.nop.dn42/
 host *.dn42.sid.mchome.nop.hu translate 3
 host *.inet.sid.mchome.nop.hu path /nfs/own/web/
 host *.inet.sid.mchome.nop.hu reconn p1 http://www.nop.hu/
 host *.inet.sid.mchome.nop.hu translate 4
 host sid.mchome.nop.hu path /nfs/own/web/
 host sid.mchome.nop.hu style table, th, td { border: 1px solid }
 host sid.mchome.nop.hu logging
 host sid.mchome.nop.hu dirlist readme stats
 host sid.mchome.nop.hu markdown
 host sid.mchome.nop.hu noindex
 host sid.mchome.nop.hu search-script log
 host sid.mchome.nop.hu script exec config
 host sid.mchome.nop.hu api exec config ipinfo show script
 host sid.mchome.nop.hu ipinfo router4 bgp4 65535
 host sid.mchome.nop.hu ipinfo router6 bgp6 65535
 host sid.mchome.nop.hu ipinfo details
 host sid.mchome.nop.hu ipinfo single
 host sid.mchome.nop.hu ipinfo style background-color:#000000;color:#00FFFF;
 host sid.mchome.nop.hu ipinfo script logger
 host sid.mchome.nop.hu ipinfo resolve
 host sid.mchome.nop.hu ipinfo others
 host sid.mchome.nop.hu websock
 host sid.mchome.nop.hu webdav
 host sid.mchome.nop.hu class
 exit
!
server ftp f vrf v1 interface loopback0
 authentication access
 path /nfs/own/web/
 exit
!
server tftp t vrf v1 interface loopback0
 path /nfs/own/web/
 exit
!
server plan9 p vrf v1 interface loopback0
 path /nfs/own/web/
 exit
!
server ntp n vrf v1 interface loopback0
 reference 0.0.0.0
 exit
!
server bmp2mrt bmp vrf v1 interface loopback0
 file bmp.log
 bulk-down
 exit
!
server dns ns vrf v1 interface loopback0
 logging
 recursion enable
 zone sid.mchome.nop.hu defttl 60
 zone sid.mchome.nop.hu axfr enable
 zone sid.mchome.nop.hu rr ip.sid.mchome.nop.hu ip4i loopback42
 zone sid.mchome.nop.hu rr sid.mchome.nop.hu ip4a 100.100.3.227
 zone sid.mchome.nop.hu rr sid.mchome.nop.hu ns ns1.sid.mchome.nop.hu
 zone sid.mchome.nop.hu rr sid.mchome.nop.hu ns ns2.sid.mchome.nop.hu
 zone sid.mchome.nop.hu rr sid.mchome.nop.hu ns ns3.sid.mchome.nop.hu
 zone sid.mchome.nop.hu rr *.sid.mchome.nop.hu cname sid.mchome.nop.hu
 zone sid.mchome.nop.hu rr sid.mchome.nop.hu soa ns0.sid.mchome.nop.hu cs.sid.mchome.nop.hu 20210309 60000 120000 6000000 600
 zone sid.mchome.nop.hu rr ip.sid.mchome.nop.hu ip6i loopback42
 zone sid.mchome.nop.hu rr sid.mchome.nop.hu ip6a 2001:db8:1101::227:227
 exit
!
server honeypot hp1 vrf v1 interface loopback0
 port 8881
 tiny-http
 info pmtud 512 1024 666
 info router4 bgp4 65535
 info router6 bgp6 65535
 info single
 info style background-color:#000000;color:#00FFFF;
 info script logger
 exit
!
server honeypot hp2 vrf v1 interface loopback0
 port 8882
 tiny-http
 info pmtud 512 1024 666
 info router4 bgp4 65535
 info router6 bgp6 65535
 info details
 info single
 info style background-color:#000000;color:#00FFFF;
 info resolve
 exit
!
server honeypot hp3 vrf v1 interface loopback0
 port 8883
 info pmtud 512 1024 666
 info router4 bgp4 65535
 info router6 bgp6 65535
 info details
 info single
 info resolve
 exit
!
server whois as vrf v1 interface loopback0
 exit
!
server sip lab vrf v1 interface loopback0
 protocol ipv4 ipv6 tcp udp
 exit
!
server radius rad vrf v1 interface loopback0
 authentication access
 secret $w10$GV+pcgTkgqct0vAiKD2PVg==
 logging
 exit
!
server tacacs tac vrf v1 interface loopback0
 authentication access
 authorization access
 secret $w10$GV+pcgTkgqct0vAiKD2PVg==
 logging
 exit
!
client proxy p1
client domain-name mchome.nop.hu
client domain-lookup
client prefer-ipv6
client whois-server www.mchome.nop.hu
client whois-online http://bgp.he.net/AS http://ipinfo.io/AS http://bgpview.io/asn/
client pastebin http://paste.nop.hu/paster.class?data=
client name-server 100.100.3.10
client time-server www.mchome.nop.hu
client time-zone CET
client mail-server mail.mchome.nop.hu
!
end
