hostname sid
buggy
password-encrypt $v10$czNjcjN0
enable $V10$Bk45WwxyuisDgdTOjjYZq9sDdjT+BinHUXVmLBcIJUMW59DxVz0=
banner encoded  
!
logging buffered debug 10240
logging file debug zzz.log
logging syslog debug system 10.10.10.10 10.10.10.4
logging irc debug irc.mchome.nop.hu #routers
!
crypto rsakey rsa import  
!
crypto dsakey dsa import  
!
crypto ecdsakey ecdsa import MEQCAQEEEACtT1ZwRkfDhndc4zXN/1GgBwYFK4EEAByhJAMiAASucERsdb81h9FyhNEdSrMbnK55VVz3W22q6dz+ggcGQA==
!
crypto certificate dsa import dsa dsa  
!
crypto certificate ecdsa import ecdsa ecdsa MIHlMIGOoAMCAQICBHdcELYwCQYHKoZIzj0EATAOMQwwCgYDVQQDEwNydHIwHhcNMTQxMDIzMDc1NjQ4WhcNMjQxMDIwMDc1NjQ4WjAOMQwwCgYDVQQDEwNydHIwNjAQBgcqhkjOPQIBBgUrgQQAHAMiAASucERsdb81h9FyhNEdSrMbnK55VVz3W22q6dz+ggcGQDAJBgcqhkjOPQQBA0cAMEQCEQCj1kFVhYyMmgeEsIMMCTalAi8Wvrl1ZghtS9ybZuiheuKZCFHKHPDOWPd4C6dKxyvvBsLep0GvqeRn/Un7+8QB0w==
!
crypto certificate rsa import rsa rsa  
!
aaa userlist access
 no log-error
 username mc36
 username mc36 password $w10$HFepawSJgqct0vAiKD2PVg==
 exit
!
access-list all4
 sequence 10 permit all any all any all
 exit
!
access-list all6
 sequence 10 permit all any all any all
 exit
!
access-list fs4
 sequence 10 permit 12-13 10.10.10.0 255.255.255.0 179 10.10.255.0 255.255.255.128 25-80
 sequence 20 permit 12-13 10.10.10.0 255.255.255.0 179 10.10.254.128 255.255.255.128 179
 exit
!
access-list fs6
 sequence 10 permit 13-14 2001:db8:1101:: ffff:ffff:ffff:ffff:: 179 2001:db8:1101:123:: ffff:ffff:ffff:ffff:ff00:: 25-80
 sequence 20 permit 13-14 2001:db8:1101:: ffff:ffff:ffff:ffff:: 179 2001:db8:1101:123:100:: ffff:ffff:ffff:ffff:ff00:: 179
 exit
!
prefix-list all
 sequence 10 permit 0.0.0.0/0 ge 0 le 32
 sequence 20 permit ::/0 ge 0 le 128
 exit
!
route-map count4
 sequence 10 action permit
 sequence 10 match network 0.0.0.0/0 ge 32 le 32
 !
 exit
!
route-map count6
 sequence 10 action permit
 sequence 10 match network ::/0 ge 128 le 128
 !
 exit
!
route-policy nht4
 sequence 10 if network 0.0.0.0/0 ge 0 le 0
 sequence 20   drop
 sequence 30 elsif distance 70
 sequence 40   pass
 sequence 50 elsif distance 0
 sequence 60   pass
 sequence 70 enif
 exit
!
route-policy nht6
 sequence 10 if network ::/0 ge 0 le 0
 sequence 20   drop
 sequence 30 elsif distance 70
 sequence 40   pass
 sequence 50 elsif distance 0
 sequence 60   pass
 sequence 70 enif
 exit
!
policy-map fs4
 sequence 10 action transit
 sequence 10 match access-group fs4
 sequence 10 match length 123-321
 sequence 10 access-rate 512000
 !
 sequence 20 action transit
 sequence 20 match length 3333-4444
 sequence 20 access-rate 768000
 !
 exit
!
policy-map fs6
 sequence 10 action transit
 sequence 10 match access-group fs6
 sequence 10 match length 123-321
 sequence 10 access-rate 512000
 !
 sequence 20 action transit
 sequence 20 match length 3333-4444
 sequence 20 access-rate 768000
 !
 exit
!
bridge 1
 rd 65535:1
 rt-import 65535:1
 rt-export 65535:1
 mac-learn
 mac-move
 private-bridge
 exit
!
bridge 2
 rd 65535:2
 rt-import 65535:2
 rt-export 65535:2
 mac-learn
 mac-move
 private-bridge
 exit
!
bridge 3
 rd 65535:1
 rt-import 65535:1
 rt-export 65535:1
 mac-learn
 mac-move
 private-bridge
 exit
!
bridge 4
 rd 65535:2
 rt-import 65535:2
 rt-export 65535:2
 mac-learn
 mac-move
 private-bridge
 exit
!
bridge 9
 mac-learn
 inspect mac
 mac-move
 exit
!
vrf definition bvi
 rd 65535:2
 label-mode per-prefix
 exit
!
vrf definition dn42
 rd 65535:42
 rt-import 65535:42
 rt-export 65535:42
 source4route all4
 source6route all6
 mdt4
 mdt6
 exit
!
vrf definition v1
 rd 1:1
 rt-import 1:1
 rt-export 1:1
 label-mode per-prefix
 source4route all4
 source6route all6
 counter4map count4
 counter6map count6
 exit
!
vrf definition v2
 rd 1:2
 rt-import 1:2
 rt-export 1:2
 label-mode per-prefix
 source4route all4
 source6route all6
 exit
!
vrf definition v3
 rd 1:3
 rt-import 1:3
 rt-export 1:3
 label-mode per-prefix
 source4route all4
 source6route all6
 exit
!
vrf definition v4
 rd 1:4
 rt-import 1:4
 rt-export 1:4
 label-mode per-prefix
 source4route all4
 source6route all6
 exit
!
vrf definition v5
 rd 1:2
 rt-import 1:2
 rt-export 1:2
 label-mode per-prefix
 source4route all4
 source6route all6
 exit
!
vrf definition vpn
 rd 65535:1
 rt-import 65535:1
 rt-export 65535:1
 label-mode per-prefix
 mdt4
 mdt6
 exit
!
vrf definition vv
 rd 1:1
 rt-import 1:1
 rt-export 1:1
 label-mode per-prefix
 exit
!
router lsrp4 1
 vrf v1
 router-id 10.10.10.227
 refresh 60000
 lifetime 2147483000
 segrout 300 299
 bier 256 300 299
 justadvert loopback0
 exit
!
router lsrp6 1
 vrf v1
 router-id 10.10.10.227
 refresh 60000
 lifetime 2147483000
 segrout 300 299
 bier 256 300 299
 justadvert loopback0
 exit
!
router logger4 1
 vrf v1
 flapstat
 redistribute bgp4 1
 exit
!
router logger6 1
 vrf v1
 flapstat
 redistribute bgp6 1
 exit
!
router deaggr4 1
 vrf v1
 justadvert bvi9
 exit
!
router deaggr6 1
 vrf v1
 justadvert bvi9
 exit
!
router mobile4 1
 vrf v1
 justadvert bvi9
 exit
!
router mobile6 1
 vrf v1
 justadvert bvi9
 exit
!
interface loopback0
 no description
 vrf forwarding v1
 ipv4 address 10.10.10.227 255.255.255.255
 ipv4 pim enable
 ipv4 pim bier-tunnel 299
 ipv4 pim join-source loopback0
 ipv6 address 2001:db8:1101::227:227 ffff:ffff:ffff:ffff:ffff:ffff:ffff:ffff
 ipv6 pim enable
 ipv6 pim bier-tunnel 299
 ipv6 pim join-source loopback0
 mpls rsvp4
 mpls rsvp6
 no shutdown
 no log-link-change
 exit
!
interface loopback42
 description dn42.net
 vrf forwarding dn42
 ipv4 address 172.23.199.109 255.255.255.255
 ipv6 address fd40:cc1e:c0de:ffff:ffff:ffff:ffff:fffd ffff:ffff:ffff:ffff:ffff:ffff:ffff:ffff
 no shutdown
 no log-link-change
 exit
!
interface loopback6
 no description
 vrf forwarding vv
 ipv4 address 1.1.1.227 255.255.255.255
 ipv6 address 1234::227 ffff:ffff:ffff:ffff:ffff:ffff:ffff:ffff
 no shutdown
 no log-link-change
 exit
!
interface loopback65535
 no description
 vrf forwarding vpn
 ipv4 address 172.16.27.4 255.255.255.255
 ipv6 address fd42:1234::4 ffff:ffff:ffff:ffff:ffff:ffff:ffff:ffff
 no shutdown
 no log-link-change
 exit
!
interface bvi1
 no description
 lldp enable
 cdp enable
 no shutdown
 no log-link-change
 exit
!
interface bvi2
 no description
 lldp enable
 cdp enable
 no shutdown
 no log-link-change
 exit
!
interface bvi3
 no description
 lldp enable
 cdp enable
 vrf forwarding bvi
 ipv4 address 2.2.2.1 255.255.255.0
 no shutdown
 no log-link-change
 exit
!
interface bvi4
 no description
 lldp enable
 cdp enable
 no shutdown
 no log-link-change
 exit
!
interface bvi9
 no description
 monitor-buffer 10240000
 cdp enable
 cdp odr4 10.1.123.91
 cdp odr6 2001:db8:1123::91
 ptp enable
 ptp receive
 carrier-delay 123
 vrf forwarding v1
 ipv4 address 10.1.123.91 255.255.255.0
 ipv4 host-watch
 ipv4 ptp enable
 ipv4 ptp receive
 ipv4 bfd 1000 3000 3
 ipv4 pim enable
 ipv4 pim bier-tunnel 299
 ipv4 pim join-source loopback0
 ipv6 address 2001:db8:1123::91 ffff:ffff:ffff:ffff::
 ipv6 host-watch
 ipv6 ptp enable
 ipv6 ptp receive
 ipv6 bfd 1000 3000 3
 ipv6 pim enable
 ipv6 pim bier-tunnel 299
 ipv6 pim join-source loopback0
 mpls enable
 mpls inspect
 mpls rsvp4
 mpls rsvp6
 router lsrp4 1 enable
 router lsrp4 1 bfd
 router lsrp6 1 enable
 router lsrp6 1 bfd
 no shutdown
 log-link-change
 exit
!
interface ethernet1
 no description
 bridge-group 9
 bridge-filter ipv4in all4
 bridge-filter ipv6in all6
 no shutdown
 no log-link-change
 exit
!
router bgp4 1
 vrf v1
 local-as 1
 router-id 10.10.10.227
 address-family unicast multicast flowspec vpnuni vpnmlt vpnflw ovpnuni ovpnmlt ovpnflw vpls mspw evpn mdt mvpn
 scandelay 30000
 conquer
 nexthop route-policy nht4
 flowspec fs4
 monitor a p1 10.10.10.227 17971
 dump a bgp4cur.log 600000 bgp4old.log
 template a remote-as 1
 no template a description
 template a password $w10$DlOpZQKK5act0vAiKD2PVg==
 template a local-as 1
 template a address-family unicast multicast other flowspec vpnuni vpnmlt vpnflw ovpnuni ovpnmlt ovpnflw vpls mspw evpn mdt mvpn
 template a distance 200
 template a compression both
 template a buffer-size 1024000
 template a ttl-security 123
 template a additional-path-rx unicast multicast other flowspec vpnuni vpnmlt vpnflw ovpnuni ovpnmlt ovpnflw vpls mspw evpn mdt mvpn
 template a additional-path-tx unicast multicast other flowspec vpnuni vpnmlt vpnflw ovpnuni ovpnmlt ovpnflw vpls mspw evpn mdt mvpn
 template a update-source loopback0
 template a monitor a
 template a dump a
 template a hostname
 template a unidirection
 template a fall-over
 template a aigp
 template a traffeng
 template a pmsitun
 template a tunenc
 template a attribset
 template a segrout
 template a bier
 template a route-reflector-client
 template a send-community all
 neighbor 10.10.10.32 template a
 neighbor 10.10.10.33 template a
 neighbor 10.10.10.34 template a
 neighbor 10.10.10.35 template a
 neighbor 10.10.10.36 template a
 neighbor 10.10.10.37 template a
 neighbor 10.10.10.91 template a
 neighbor 10.10.10.92 template a
 neighbor 10.10.10.93 template a
 neighbor 10.10.10.94 template a
 neighbor 10.10.10.95 template a
 neighbor 10.10.10.96 template a
 neighbor 10.10.10.225 template a
 neighbor 10.10.10.226 template a
 neighbor 10.10.10.228 template a
 neighbor 10.10.10.229 template a
 afi-vrf vv enable
 afi-vrf vv flowspec fs4
 afi-vrf vv mvpn loopback0
 afi-vrf vv redistribute connected
 afi-ovrf vv enable
 afi-ovrf vv flowspec fs6
 afi-ovrf vv mvpn loopback0
 afi-ovrf vv redistribute connected
 redistribute connected
 exit
!
router bgp4 65535
 vrf v1
 local-as 65535
 router-id 10.10.10.227
 address-family labeled multicast other flowspec vpnuni vpnmlt vpnflw ovpnuni ovpnmlt ovpnflw vpls mspw evpn mdt mvpn omvpn
 flapstat
 dump mrt bgp1.log
 neighbor 10.5.1.10 remote-as 65535
 no neighbor 10.5.1.10 description
 neighbor 10.5.1.10 local-as 65535
 neighbor 10.5.1.10 address-family labeled multicast other flowspec vpnuni vpnmlt vpnflw ovpnuni ovpnmlt ovpnflw vpls mspw evpn mdt mvpn omvpn
 neighbor 10.5.1.10 distance 200
 neighbor 10.5.1.10 compression both
 neighbor 10.5.1.10 update-source loopback0
 neighbor 10.5.1.10 dump mrt
 neighbor 10.5.1.10 hostname
 neighbor 10.5.1.10 aigp
 neighbor 10.5.1.10 traffeng
 neighbor 10.5.1.10 pmsitun
 neighbor 10.5.1.10 tunenc
 neighbor 10.5.1.10 attribset
 neighbor 10.5.1.10 segrout
 neighbor 10.5.1.10 bier
 neighbor 10.5.1.10 send-community all
 afi-vrf dn42 enable
 afi-vrf dn42 mvpn loopback0
 afi-vrf dn42 redistribute connected
 afi-vrf dn42 redistribute static
 afi-vrf vpn enable
 afi-vrf vpn mvpn loopback0
 afi-vrf vpn redistribute connected
 afi-vrf vpn redistribute static
 afi-ovrf dn42 enable
 afi-ovrf dn42 mvpn loopback0
 afi-ovrf dn42 redistribute connected
 afi-ovrf dn42 redistribute static
 afi-vpls 65535:1 bridge-group 1
 afi-vpls 65535:1 update-source loopback0
 afi-evpn 2 bridge-group 2
 afi-evpn 2 bmac 006e.085c.1743
 afi-evpn 2 encapsulation pbb
 afi-evpn 2 update-source loopback0
 redistribute connected
 redistribute static
 exit
!
router bgp6 1
 vrf v1
 local-as 1
 router-id 10.10.10.227
 address-family unicast multicast flowspec vpnuni vpnmlt vpnflw ovpnuni ovpnmlt ovpnflw vpls mspw evpn mdt mvpn
 scandelay 30000
 conquer
 nexthop route-policy nht6
 flowspec fs6
 monitor a p1 10.10.10.227 17971
 dump a bgp6cur.log 600000 bgp6old.log
 template a remote-as 1
 no template a description
 template a password $w10$DlOpZQKK5act0vAiKD2PVg==
 template a local-as 1
 template a address-family unicast multicast flowspec vpnuni vpnmlt vpnflw ovpnuni ovpnmlt ovpnflw vpls mspw evpn mdt mvpn
 template a distance 200
 template a compression both
 template a buffer-size 1024000
 template a ttl-security 123
 template a additional-path-rx unicast multicast flowspec vpnuni vpnmlt vpnflw ovpnuni ovpnmlt ovpnflw vpls mspw evpn mdt mvpn
 template a additional-path-tx unicast multicast flowspec vpnuni vpnmlt vpnflw ovpnuni ovpnmlt ovpnflw vpls mspw evpn mdt mvpn
 template a update-source loopback0
 template a monitor a
 template a dump a
 template a hostname
 template a unidirection
 template a fall-over
 template a aigp
 template a traffeng
 template a pmsitun
 template a tunenc
 template a attribset
 template a segrout
 template a bier
 template a route-reflector-client
 template a send-community all
 neighbor 2001:db8:1101::32 template a
 neighbor 2001:db8:1101::33 template a
 neighbor 2001:db8:1101::34 template a
 neighbor 2001:db8:1101::35 template a
 neighbor 2001:db8:1101::36 template a
 neighbor 2001:db8:1101::37 template a
 neighbor 2001:db8:1101::91 template a
 neighbor 2001:db8:1101::92 template a
 neighbor 2001:db8:1101::93 template a
 neighbor 2001:db8:1101::94 template a
 neighbor 2001:db8:1101::95 template a
 neighbor 2001:db8:1101::96 template a
 redistribute connected
 exit
!
router bgp6 65535
 vrf v1
 local-as 65535
 router-id 10.10.10.227
 address-family labeled multicast other flowspec vpnuni vpnmlt vpnflw ovpnuni ovpnmlt ovpnflw vpls mspw evpn mdt mvpn omvpn
 flapstat
 dump mrt bgp2.log
 neighbor 2001:db8:36::2 remote-as 65535
 no neighbor 2001:db8:36::2 description
 neighbor 2001:db8:36::2 local-as 65535
 neighbor 2001:db8:36::2 address-family labeled multicast other flowspec vpnuni vpnmlt vpnflw ovpnuni ovpnmlt ovpnflw vpls mspw evpn mdt mvpn omvpn
 neighbor 2001:db8:36::2 distance 200
 neighbor 2001:db8:36::2 compression both
 neighbor 2001:db8:36::2 update-source loopback0
 neighbor 2001:db8:36::2 dump mrt
 neighbor 2001:db8:36::2 hostname
 neighbor 2001:db8:36::2 aigp
 neighbor 2001:db8:36::2 traffeng
 neighbor 2001:db8:36::2 pmsitun
 neighbor 2001:db8:36::2 tunenc
 neighbor 2001:db8:36::2 attribset
 neighbor 2001:db8:36::2 segrout
 neighbor 2001:db8:36::2 bier
 neighbor 2001:db8:36::2 send-community all
 afi-vrf vpn enable
 afi-vrf vpn mvpn loopback0
 afi-vrf vpn redistribute connected
 afi-vrf vpn redistribute static
 afi-vpls 65535:1 bridge-group 3
 afi-vpls 65535:1 update-source loopback0
 afi-evpn 2 bridge-group 4
 afi-evpn 2 bmac 0002.4276.7a16
 afi-evpn 2 encapsulation pbb
 afi-evpn 2 update-source loopback0
 redistribute connected
 redistribute static
 exit
!
proxy-profile p1
 vrf v1
 source loopback0
 exit
!
proxy-profile p2
 vrf v2
 exit
!
proxy-profile p3
 vrf v3
 exit
!
proxy-profile p4
 vrf v4
 exit
!
proxy-profile p5
 vrf v5
 exit
!
mtracker v4
 logging
 target 10.5.1.10
 vrf v1
 source loopback0
 start
 exit
!
mtracker v4m
 logging
 target 10.5.1.10
 vrf v1
 source loopback0
 port 5488
 start
 exit
!
mtracker v6
 logging
 target 2001:db8:36::2
 vrf v1
 source loopback0
 start
 exit
!
mtracker v6m
 logging
 target 2001:db8:36::2
 vrf v1
 source loopback0
 port 5488
 start
 exit
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
ipv4 flow v1 collect
!
ipv6 flow v1 collect
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
translation-rule 1
 remove %20
 remove -
 remove \(
 remove \)
 replace \+36 06
 match ^sip:(?<n>[0-9]+)@(?<d>.*)$
 match ^.*<sip:(?<n>[0-9]+)@(?<d>.*)>.*$
 match ^(?<n>[0-9]+)$
 text "
 variable n
 text "
 character 32
 text <sip:
 variable n
 text @10.10.10.10>
 log
 exit
!
translation-rule 2
 match .*
 text "96" <sip:97@10.10.10.10>
 exit
!
dial-peer 1
 match-calling .*
 match-called .*
 translate-out-calling 2
 translate-out-called 1
 port-local 6050
 port-remote 6050
 keepalive 15000
 log
 history 10
 vrf v1
 source loopback0
 myname 97
 target 2001:db8:1101::10
 max-calls-in 99
 max-calls-out 99
 protocol sip-connect
 direction both
 exit
!
alias test bash description 
alias test bash parameter optional
!
server telnet ssh
 security protocol ssh
 security authentication access
 security rsakey rsa
 security dsakey dsa
 security ecdsakey ecdsa
 security rsacert rsa
 security dsacert dsa
 security ecdsacert ecdsa
 port 22
 no login authentication
 vrf v1
 exit
!
server telnet tel
 security protocol telnet
 exec width 80
 exec height 25
 login authentication access
 vrf v1
 exit
!
server rfb vnc
 no login authentication
 vrf v1
 exit
!
server http web
 access-log
 access-total 128
 access-peer 16
 host * path /nfs2/own/web/home/
 host * logging
 host * dirlist
 host * script
 host * websock
 host * webdav
 host * class
 vrf v1
 exit
!
server bmp2mrt bmp
 max-time 600000
 backup bmp-old.log
 file bmp-cur.log
 bulk-down
 vrf v1
 exit
!
server dns ns
 recursion enable
 vrf v1
 exit
!
server sip lab
 protocol ipv4 ipv6 tcp udp
 interface loopback0
 vrf v1
 exit
!
client proxy p1
client prefer-ipv6
client password-stars
client whois-server whois.ripe.net
client name-server 8.8.8.8
client upgrade-config
client time-zone CET
!
end
