hostname r1
buggy
!
logging file debug ../binTmp/zzz0r1-log.run
!
vrf definition tester
 exit
!
vrf definition v1
 rd 1:1
 exit
!
interface loopback0
 vrf forwarding v1
 ipv4 address 2.2.2.1 255.255.255.255
 ipv6 address 4321::1 ffff:ffff:ffff:ffff:ffff:ffff:ffff:ffff
 no shutdown
 no log-link-change
 exit
!
interface ethernet1
 description r2 e1
 lldp enable
 vrf forwarding v1
 ipv4 address 1.1.1.1 255.255.255.252
 ipv6 address 1234:1::1 ffff:ffff::
 no shutdown
 no log-link-change
 exit
!
interface ethernet2
 description r3 e2
 lldp enable
 vrf forwarding v1
 ipv4 address 1.1.1.5 255.255.255.252
 ipv6 address 1234:2::1 ffff:ffff::
 no shutdown
 no log-link-change
 exit
!
proxy-profile p1
 vrf v1
 exit
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
server telnet tel
 security protocol telnet
 no exec authorization
 no login authentication
 vrf v1
 exit
!
server telnet tester
 security protocol telnet
 no exec authorization
 no login authentication
 vrf tester
 exit
!
client proxy p1
!
end
