hostname core1
buggy
!
logging buffered debug 10240
logging file debug core1.log
!
crypto rsakey rsa import  
!
crypto dsakey dsa import MIH2AgEAAkBdHH+NJ78OHDDYJMwqqEA7/Fmyn0SPNCe3+doCqKSbwYPS7FpgIqP8R7cIv0GDzxmCPFYJIZ/pWmu0VleClF4LAhUAlTGwTPM+Vla+iYnYroywSCsBQ+MCQBmx+2JlMnQWpPj65oNafjpAXmYFVw0AqPAguzRmbS0A6XsDAygDkIFC0IX806b2lCwIvm4/nyNtY6lyxq0mi00CQDQfodwCipoFayCfWXjC7z7jTN26MXmk4oP+pgSG9aF8dG34Wrx7A/GHoTkaAwMbTbXgzlOQ5O5UtIKy04xai1UCFDK+gTIq1c/alJ2EOsvC5tvW1siW
!
crypto ecdsakey ecdsa import MIHbAgEBBEAA392naCtU5jkwV+4yD1PBoFODWiOqRdA3Mej7Buh+NOrlsgq/6R0p1CND6Rf+EyYARnsYvMBLD/msqdFczUZvoAwGCgEDJAMDAggBAQ2hgYUDgYIABCZQjKVjdcoDTm5Mwvf+IOeYAZ7+ptlG7cGxPZGXj5saqQDMNB+Jnj0sck0s+rsTDwP3wt/0BFv14Fm35kU8W+gUrlYtFQ/ZKy88cuAGy3z1UeSWVErszXYDaBLmFyb+H7/LfO9bIfDtHxJ30XyXpAlmLCKRywfxnXrrqLuxLEez
!
aaa userlist usr
 no log-error
 username rare
 username rare password $v10$cmFyZQ==
 exit
!
bundle 1
 exit
!
vrf definition v1
 rd 1:1
 rt-import 1:1
 rt-export 1:1
 label-mode per-prefix
 exit
!
router isis4 1
 vrf v1
 net-id 49.0001.0000.0a01.0101.00
 traffeng-id ::
 is-type level1
 segrout 10
 level1 segrout
 exit
!
interface loopback0
 no description
 vrf forwarding v1
 ipv4 address 10.1.1.1 255.255.255.255
 router isis4 1 enable
 router isis4 1 passive
 router isis4 1 circuit level1
 router isis4 1 segrout index 1
 no shutdown
 no log-link-change
 exit
!
interface bundle1
 no description
 vrf forwarding v1
 ipv4 address 10.1.2.1 255.255.255.0
 mpls enable
 router isis4 1 enable
 router isis4 1 circuit level1
 no shutdown
 no log-link-change
 exit
!
interface ethernet0
 no description
 macaddr 0000.0a00.0040
 no shutdown
 no log-link-change
 exit
!
interface sdn1
 no description
 mtu 1500
 macaddr 0006.0b5a.2340
 bundle-group 1
 no shutdown
 no log-link-change
 exit
!
interface sdn2
 no description
 mtu 1500
 macaddr 006a.6b69.2a4f
 bundle-group 1
 no shutdown
 no log-link-change
 exit
!
interface sdn3
 no description
 mtu 1500
 macaddr 0067.1922.2a19
 no shutdown
 no log-link-change
 exit
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
server telnet ssh
 security protocol ssh
 security authentication usr
 security rsakey rsa
 security dsakey dsa
 security ecdsakey ecdsa
 port 22
 exec logging
 no exec authorization
 no login authentication
 vrf v1
 exit
!
server telnet tel
 security protocol telnet
 exec width 130
 exec height 25
 no exec authorization
 no login authentication
 vrf v1
 exit
!
server p4lang p4
 export-vrf v1 1
 export-port sdn1 128 10
 export-port sdn2 136 10
 export-port sdn3 144 10
 export-port bundle1 500 10
 interconnect ethernet0
 vrf v1
 exit
!
client name-server 8.8.8.8
client config-save
client time-zone CET
!
end
